;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Installation##OTHER##
NOTOR65 SURF/PEND D 800 HL OPAL 840_13660-20052;65;2.1;4000;1667;Acrylic - Fagerhult - Opal;840;1667;4000;4000;20;65;134;White;Aluminium - Fagerhult - White;7320049874855;13660-20052;13;13;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;1
NOTOR65 SURF/PEND D 1200 HL OPAL 840_13660-20053;65;3.5;4000;2500;Acrylic - Fagerhult - Opal;1256;2500;4000;4000;20;65;149;White;Aluminium - Fagerhult - White;7320049874886;13660-20053;18;18;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;1
NOTOR65 SURF/PEND D 2400 HL OPAL 840_13660-20054;65;6.4;4000;5000;Acrylic - Fagerhult - Opal;2506;5000;4000;4000;20;65;149;White;Aluminium - Fagerhult - White;7320049874916;13660-20054;36;36;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;1
NOTOR65 SURF/PEND D 800 HL OPAL 840_13660-21008;65;2.1;4000;1667;Acrylic - Fagerhult - Opal;840;1667;4000;4000;20;65;134;White;Aluminium - Fagerhult - White;7316911856104;13660-21008;13;13;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;1
NOTOR65 SURF/PEND D 1200 HL OPAL 840_13660-21012;65;3.5;4000;2500;Acrylic - Fagerhult - Opal;1256;2500;4000;4000;20;65;149;White;Aluminium - Fagerhult - White;7316911856593;13660-21012;18;18;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;1
NOTOR65 SURF/PEND D 2400 HL OPAL 840_13660-21016;65;6.4;4000;5000;Acrylic - Fagerhult - Opal;2506;5000;4000;4000;20;65;149;White;Aluminium - Fagerhult - White;7316911855640;13660-21016;36;36;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;1
NOTOR65 SURF/PEND D 800 HL OPAL 840_13660-21020;65;2;4000;1667;Acrylic - Fagerhult - Opal;836;1667;4000;4000;20;65;134;White;Aluminium - Fagerhult - White;7316911855770;13660-21020;13;13;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;2
NOTOR65 SURF/PEND D 1200 HL OPAL 840_13660-21024;65;3.4;4000;2500;Acrylic - Fagerhult - Opal;1252;2500;4000;4000;20;65;149;White;Aluminium - Fagerhult - White;7316911856609;13660-21024;18;18;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;2
NOTOR65 SURF/PEND D 2400 HL OPAL 840_13660-21028;65;6.3;4000;5000;Acrylic - Fagerhult - Opal;2502;5000;4000;4000;20;65;149;White;Aluminium - Fagerhult - White;7316911857064;13660-21028;36;36;Notor 65 Opal;Single or continuous installation via wire suspension or surface mounted. Installation via wire suspension requires wire brackets which provide flexible c/c, see accessories. Can also be wall mounted with special brackets, see Accessories.;Suspended or ceiling mounted with direct light only via Opal louvres. Single or continuous installation.;min. 80;C;1;2
