;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Louvre##OTHER##;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##;Lamell Length##OTHER##;Organic Respons##OTHER##
DTI TYPE1 1000LM 600 WHITE 3K_29460;141;2.8;3000;900;Aluminium - Fagerhult - Beta Opti;765;900;3000;3000;20;59;110;White;Steel - Fagerhult - White;7320046220204;29460;8;8;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
DTI TYPE1 1000LM 600 WHITE 3K_29460-402;141;2.8;3000;900;Aluminium - Fagerhult - Beta Opti;765;900;3000;3000;20;59;114;White;Steel - Fagerhult - White;7320046220228;29460-402;8.5;8.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
DTI TYPE1 2000LM 1200 WHITE 3K_29461;141;2.8;3000;1970;Aluminium - Fagerhult - Beta Opti;1365;1970;3000;3000;20;59;131;White;Steel - Fagerhult - White;7320046220242;29461;15;15;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2000LM 1200 WHITE 3K_29461-402;141;2.8;3000;1970;Aluminium - Fagerhult - Beta Opti;1365;1970;3000;3000;20;59;136;White;Steel - Fagerhult - White;7320046220266;29461-402;15.5;15.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2900LM 1200 WHITE 3K_29462;141;2.8;3000;2934;Aluminium - Fagerhult - Beta Opti;1365;2934;3000;3000;20;59;135;White;Steel - Fagerhult - White;7320046220280;29462;22;22;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2900LM 1200 WHITE 3K_29462-402;141;2.8;3000;2934;Aluminium - Fagerhult - Beta Opti;1365;2934;3000;3000;20;59;139;White;Steel - Fagerhult - White;7320046220303;29462-402;22;22;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2900LM 1200 WHITE 3K_29462-533;141;2.8;3000;2900;Aluminium - Fagerhult - Beta Opti;1365;2900;3000;3000;20;59;121;White;Steel - Fagerhult - White;7,32005E+12;29462-533;24;24;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
DTI TYPE1 3700LM 1200 WHITE 3K UGR19_29463;141;2.8;3000;3755;Aluminium - Fagerhult - Beta Opti;1365;3755;3000;3000;20;59;125;White;Steel - Fagerhult - White;7320046220327;29463;30;30;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 3700LM 1200 WHITE 3K UGR19_29463-402;141;2.8;3000;3711;Aluminium - Fagerhult - Beta Opti;1365;3711;3000;3000;20;59;130;White;Steel - Fagerhult - White;7320046242015;29463-402;30.5;30.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 3700LM 1200 WHITE 3K UGR19_29463-515;141;2.8;3000;3755;Aluminium - Fagerhult - Beta Opti;1365;3755;3000;3000;20;59;121;White;Steel - Fagerhult - White;7320046688820;29463-515;31;31;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 3700LM 1200 WHITE 3K UGR19_29463-537;141;2.8;3000;3711;Aluminium - Fagerhult - Beta Opti;1365;3711;3000;3000;20;59;124;White;Steel - Fagerhult - White;7320047651984;29463-537;30.5;30.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 3K_29464;141;2.8;3000;5348;Aluminium - Fagerhult - Beta Opti;1365;5348;3000;3000;20;59;134;White;Steel - Fagerhult - White;7320046220389;29464;40;40;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 3K_29464-402;141;2.8;3000;5348;Aluminium - Fagerhult - Beta Opti;1365;5348;3000;3000;20;59;132;White;Steel - Fagerhult - White;7320046220402;29464-402;42.5;42.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 3K_29464-515;141;2.8;3000;5348;Aluminium - Fagerhult - Beta Opti;1365;5348;3000;3000;20;59;130;White;Steel - Fagerhult - White;7320046688837;29464-515;41;41;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 3K_29464-537;141;2.8;3000;5348;Aluminium - Fagerhult - Beta Opti;1365;5348;3000;3000;20;59;132;White;Steel - Fagerhult - White;7320047652165;29464-537;42.5;42.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 1000LM 600 WHITE 4K_29465;141;2.8;4000;926;Aluminium - Fagerhult - Beta Opti;765;926;4000;4000;20;59;113;White;Steel - Fagerhult - White;7320046220440;29465;8;8;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
DTI TYPE1 1000LM 600 WHITE 4K_29465-402;141;2.8;4000;926;Aluminium - Fagerhult - Beta Opti;765;926;4000;4000;20;59;117;White;Steel - Fagerhult - White;7320046220464;29465-402;8.5;8.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;1;0
DTI TYPE1 2000LM 1200 WHITE 4K_29466;141;2.8;4000;2027;Aluminium - Fagerhult - Beta Opti;1365;2027;4000;4000;20;59;135;White;Steel - Fagerhult - White;7320046220488;29466;15;15;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2000LM 1200 WHITE 4K_29466-402;141;2.8;4000;2027;Aluminium - Fagerhult - Beta Opti;1365;2027;4000;4000;20;59;140;White;Steel - Fagerhult - White;7320046220501;29466-402;15.5;15.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2900LM 1200 WHITE 4K_29467;141;2.8;4000;3019;Aluminium - Fagerhult - Beta Opti;1365;3019;4000;4000;20;59;139;White;Steel - Fagerhult - White;7320046220525;29467;22;22;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2900LM 1200 WHITE 4K_29467-402;141;2.8;4000;3019;Aluminium - Fagerhult - Beta Opti;1365;3019;4000;4000;20;59;143;White;Steel - Fagerhult - White;7320046220549;29467-402;22;22;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 2900LM 1200 WHITE 4K_29467-533;141;2.8;4000;3019;Aluminium - Fagerhult - Beta Opti;1365;3019;4000;4000;20;59;135;White;Steel - Fagerhult - White;7320047806346;29467-533;23.5;23.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
DTI TYPE1 3900LM 1200 WHITE 4K UGR19_29468;141;2.8;4000;3864;Aluminium - Fagerhult - Beta Opti;1365;3864;4000;4000;20;59;129;White;Steel - Fagerhult - White;7320046220563;29468;30;30;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 3900LM 1200 WHITE 4K UGR19_29468-402;141;2.8;4000;3818;Aluminium - Fagerhult - Beta Opti;1365;3818;4000;4000;20;59;133;White;Steel - Fagerhult - White;7320046242008;29468-402;30.5;30.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 3900LM 1200 WHITE 4K UGR19_29468-515;141;2.8;4000;3864;Aluminium - Fagerhult - Beta Opti;1365;3864;4000;4000;20;59;125;White;Steel - Fagerhult - White;7320046688844;29468-515;31;31;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 3900LM 1200 WHITE 4K UGR19_29468-537;141;2.8;4000;3818;Aluminium - Fagerhult - Beta Opti;1365;3818;4000;4000;20;59;129;White;Steel - Fagerhult - White;7320047652141;29468-537;31.5;31.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 4K_29469;141;2.8;4000;5503;Aluminium - Fagerhult - Beta Opti;1365;5503;4000;4000;20;59;137;White;Steel - Fagerhult - White;7320046220624;29469;40;40;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 4K_29469-402;141;2.8;4000;5503;Aluminium - Fagerhult - Beta Opti;1365;5503;4000;4000;20;59;136;White;Steel - Fagerhult - White;7320046220648;29469-402;42.5;42.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 5200LM 1200 WHITE 4K_29469-515;141;2.8;4000;5503;Aluminium - Fagerhult - Beta Opti;1365;5503;4000;4000;20;59;134;White;Steel - Fagerhult - White;7320046688851;29469-515;41;41;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;0
DTI TYPE1 4900LM 1500 WHITE 4K UGR19_29667;141;2.8;4000;4721;Aluminium - Fagerhult - Beta Opti;1665;4721;4000;4000;20;59;131;White;Steel - Fagerhult - White;7320046415716;29667;36;36;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
DTI TYPE1 4900LM 1500 WHITE 4K UGR19_29667-402;141;2.8;4000;4778;Aluminium - Fagerhult - Beta Opti;1665;4778;4000;4000;20;59;134;White;Steel - Fagerhult - White;7320046600808;29667-402;37.5;37.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
DTI TYPE1 4700LM 1500 WHITE 3K UGR19_29669;141;2.8;3000;4590;Aluminium - Fagerhult - Beta Opti;1665;4590;3000;3000;20;59;134;White;Steel - Fagerhult - White;7320046600419;29669;35;35;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
DTI TYPE1 4700LM 1500 WHITE 3K UGR19_29669-402;141;2.8;3000;4644;Aluminium - Fagerhult - Beta Opti;1665;4644;3000;3000;20;59;130;White;Steel - Fagerhult - White;7320046600426;29669-402;37.5;37.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;3;0
DTI TYPE1 3700LM 1200 WHITE 3K UGR19_29463-546;141;2.9;3000;3672;Aluminium - Fagerhult - Beta Opti;1365;3672;3000;3000;20;59;122;White;Steel - Fagerhult - White;7320048522047;29463-546;31;31;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
DTI TYPE1 3900LM 1200 WHITE 4K UGR19_29468-546;141;2.9;4000;3778;Aluminium - Fagerhult - Beta Opti;1365;3778;4000;4000;20;59;126;White;Steel - Fagerhult - White;7320048522054;29468-546;31;31;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
DTI TYPE1 5200LM 1200 WHITE 3K_29464-533;141;2.8;3000;5348;Aluminium - Fagerhult - Beta Opti;1365;5348;3000;3000;20;59;128;White;Steel - Fagerhult - White;7316910929991;29464-533;44.5;44.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
DTI TYPE1 5200LM 1200 WHITE 4K_29469-533;141;2.8;4000;5503;Aluminium - Fagerhult - Beta Opti;1365;5503;4000;4000;20;59;132;White;Steel - Fagerhult - White;7316910621635;29469-533;44.5;44.5;DTI LED Type 1;Surface mounted or wire suspension. Installation via wire suspension requires wire suspension and wire bracket 91685, see accessories.;A ceiling-mounted workplace luminaire. Beta Opti louvres provide high efficiency and optimal lighting comfort.;min. 80;C;1;2;1
