;Width##LENGTH##MILLIMETERS;Weight (Kg)##OTHER##;Temperature Color##OTHER##;Luminous Flux##ELECTRICAL_LUMINOUS_FLUX##LUMENS;Length##LENGTH##MILLIMETERS;Initial Intensity##OTHER##;Initial Color Temperature##COLOR_TEMPERATURE##KELVIN;Initial Color##OTHER##;IP Code##OTHER##;Height##LENGTH##MILLIMETERS;Efficacy##ELECTRICAL_EFFICACY##LUMENS_PER_WATT;Color##OTHER##;Body##OTHER##;EAN_Code##OTHER##;Article Number##OTHER##;Wattage##ELECTRICAL_WATTAGE##WATTS;Apparent Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES;Model##OTHER##;Type Comments##OTHER##;Description##OTHER##;Color Rendering Index##Other##;Energy Class##OTHER##;BIM Version##OTHER##
HERO 12KLM MEDIUM 4000K HTG_31500;307;7.3;4000;12183;498;12183;4000;4000;66;87;149;Black;Fagerhult_Black_aluminium;7320046433505;31500;82;82;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 12KLM MEDIUM 4000K HTG_31500-461;307;7.3;4000;12183;498;12183;4000;4000;66;87;150;Black;Fagerhult_Black_aluminium;7320046433529;31500-461;81;81;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 12KLM MEDIUM 4000K HTG_31500-526;307;7.3;4000;12183;589;12183;4000;4000;65;102;148;Black;Fagerhult_Black_aluminium;7320047242939;31500-526;83;83;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 18KLM MEDIUM 4000K HTG_31503;307;7.3;4000;18157;498;18157;4000;4000;66;87;143;Black;Fagerhult_Black_aluminium;7320046433772;31503;127;127;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 18KLM MEDIUM 4000K HTG_31503-461;307;7.3;4000;18157;498;18157;4000;4000;66;87;145;Black;Fagerhult_Black_aluminium;7320046433796;31503-461;126;126;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 24KLM MEDIUM 4000K HTG_31506-461;307;7.3;4000;23987;498;23987;4000;4000;66;87;154;Black;Fagerhult_Black_aluminium;7320046434021;31506-461;156;156;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 24KLM MEDIUM 4000K HTG_31506-526;307;7.3;4000;23987;589;23987;4000;4000;65;102;153;Black;Fagerhult_Black_aluminium;7320047243059;31506-526;157;157;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 12KLM MEDIUM 4000K PMMA_31510;307;7.3;4000;12146;498;12146;4000;4000;66;87;148;Black;Fagerhult_Black_aluminium;7320046433536;31510;82;82;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 12KLM MEDIUM 4000K PMMA_31510-461;307;7.3;4000;12146;498;12146;4000;4000;66;87;150;Black;Fagerhult_Black_aluminium;7320046433567;31510-461;81;81;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 12KLM MEDIUM 4000K PMMA_31510-526;307;7.3;4000;12146;589;12146;4000;4000;65;102;147;Black;Fagerhult_Black_aluminium;7320047242946;31510-526;83;83;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 18KLM MEDIUM 4000K PMMA_31513;307;7.3;4000;18103;498;18103;4000;4000;66;87;143;Black;Fagerhult_Black_aluminium;7320046433802;31513;127;127;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 18KLM MEDIUM 4000K PMMA_31513-461;307;7.3;4000;18103;498;18103;4000;4000;66;87;144;Black;Fagerhult_Black_aluminium;7320046433826;31513-461;126;126;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 18KLM MEDIUM 4000K PMMA_31513-526;307;7.3;4000;18103;589;18103;4000;4000;65;102;143;Black;Fagerhult_Black_aluminium;7320047243004;31513-526;127;127;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 24KLM MEDIUM 4000K PMMA_31516;307;7.3;4000;23915;498;23915;4000;4000;66;87;149;Black;Fagerhult_Black_aluminium;7320046434038;31516;161;161;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 24KLM MEDIUM 4000K PMMA_31516-461;307;7.3;4000;23915;498;23915;4000;4000;66;87;153;Black;Fagerhult_Black_aluminium;7320046434052;31516-461;156;156;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 24KLM MEDIUM 4000K PMMA_31516-526;307;7.3;4000;23915;589;23915;4000;4000;65;102;152;Black;Fagerhult_Black_aluminium;7320047243066;31516-526;157;157;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 18KLM MEDIUM 4000K HTG_31503-526;307;7.3;4000;18157;589;18157;4000;4000;65;102;143;Black;Fagerhult_Black_aluminium;7320047242991;31503-526;127;127;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
HERO 24KLM MEDIUM 4000K HTG_31506;307;7.3;4000;23987;498;23987;4000;4000;66;87;150;Black;Fagerhult_Black_aluminium;7320046434007;31506;161;161;Hero Medium Beam;Flush-mounted, surface-mounted tandem bracket, tube bracket, wire bracket, adjustable ceiling/wall bracket and recess frame. Installation accessories are ordered separately, see accessories.;Developed for industrial facilities or sports centres with ball protection certification per VDE 0710-13. Glare-free with different lumen packages and provides a good, glare-free light even from greater heights.;min. 80;E;1
